{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Orders2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Orders2","index":0,"n_rows":33,"n_cols":17,"rows_kept":33,"cut":false,"hidden":false,"merged":[[28,1,28,13],[30,1,30,13],[1,1,1,6],[1,7,1,13],[5,1,5,13],[21,1,21,13],[25,1,25,13]]}
[]
[null,"Обязательные поля (в строгом порядке)",null,null,null,null,null,"Не обязательные поля (в любом порядке)"]
[null,"тип элемента","ID","Виджет","Имя вкладки","Имя виджета","Позиция виджета","адрес сенсора","номер пина","масштабирование","коррекция","инверсия","начальное состояние","дребезг мили секунды"]
[null,null,"Это имя должно быть уникально, и должно состоять из английских букв, оно необходимо для обращения к элементу из сценариев","Виджет который будет отображать информацию","Название вкладки в приложении","Название виджета в приложении","Этот номер нужен для определения порядка виджетов на экране ","Адрес сенсора i2c. Этот адрес можно получить воспользовавшись i2c сканером в утилитах","Номера пинов соответствуют оффициальным номерам gpio esp ","Преобразование выходного значения датчика из одного диапазона в другой","Сюда вводится коэффициент поправки на который будет умножено значение сенсора","Если нужно запустить инверсию кнопки (Во включенном будет low в выключенном high)","Здесь задаются все начальные состояния","Дребизг физической кнопки"]
[null,"id","key","file","page","descr","order","addr","pin","map","c","inv","state","db"]
[null,"Сенсоры",null,null,null,null,null,null,null,null,null,null,null,null,null,null," Сенсоры"]
[null,"usonic-pr","usonic-pr","fillgauge","Сенсоры","Уровень",1,null,"pin[14,15]","map[1,100,1,100]","c[0]",null,null,null,0,null," ultrasonic-pr pr fillgauge Сенсоры Уровень 1 pin[14,15] map[1,100,1,100] c[0]"]
[null,"usonic-cm","usonic-cm","fillgauge","Сенсоры","Расстояние",2,null,"pin[14]",null,null,null,null,null,0,null," ultrasonic-cm cm fillgauge Сенсоры Расстояние 2 pin[14]"]
[null,"analog-adc","analog-adc","any-data","Сенсоры","Аналоговый",3,null,"pin[2]","map[1,100,1,100]",null,null,null,null,0,null," analog-adc adc any-data Сенсоры Аналоговый 3 pin[2] map[1,100,1,100]"]
[null,"dallas-temp","dallas-temp","any-data","Сенсоры","Температура",4,null,"pin[2]",null,null,null,null,null,0,null," dallas-temp tDal any-data Сенсоры Температура 4 pin[2]"]
[null,"dht11-temp","dht11-temp","any-data","Сенсоры","Температура",5,null,"pin[2]",null,null,null,null,null,0,null," dht11-temp tDht any-data Сенсоры Температура 5 pin[2]"]
[null,"dht11-hum","dht11-hum","any-data","Сенсоры","Влажность",6,null,"pin[2]",null,null,null,null,null,0,null," dht11-hum hDht any-data Сенсоры Влажность 6 pin[2]"]
[null,"dht11-perc","dht11-perc","any-data","Сенсоры","Восприятие",7,null,"pin[2]",null,null,null,null,null,0,null," dht11-perc pDht any-data Сенсоры Восприятие 7 pin[2]"]
[null,"dht11-com","dht11-com","any-data","Сенсоры","Комфорт",8,null,"pin[2]",null,null,null,null,null,0,null," dht11-com cDht any-data Сенсоры Комфорт 8 pin[2]"]
[null,"dht11-dew","dht11-dew","any-data","Сенсоры","Точка росы",9,null,"pin[2]",null,null,null,null,null,0,null," dht11-dew dDht any-data Сенсоры Точка росы 9 pin[2]"]
[null,"bmp280-temp","bmp280-temp","any-data","Сенсоры","Температура",10,"addr[0x25]",null,null,null,null,null,null,0,null," bmp280-temp tBmp any-data Сенсоры Температура 10 addr[0x25]"]
[null,"bmp280-press","bmp280-press","any-data","Сенсоры","Давление",11,"addr[0x25]",null,null,null,null,null,null,0,null," bmp280-press pBmp any-data Сенсоры Давление 11 addr[0x25]"]
[null,"bme280-temp","bme280-temp","any-data","Сенсоры","Температура",12,"addr[0x25]",null,null,null,null,null,null,0,null," bme280-temp tBme any-data Сенсоры Температура 12 addr[0x25]"]
[null,"bme280-press","bme280-press","any-data","Сенсоры","Давление",13,"addr[0x25]",null,null,null,null,null,null,0,null," bme280-press pBme any-data Сенсоры Давление 13 addr[0x25]"]
[null,"bme280-hum","bme280-hum","any-data","Сенсоры","Влажность",14,"addr[0x25]",null,null,null,null,null,null,0,null," bme280-hum hBme any-data Сенсоры Влажность 14 addr[0x25]"]
[null,"bme280-alt","bme280-alt","any-data","Сенсоры","Высота",15,"addr[0x25]",null,null,null,null,null,null,0,null," bme280-alt aBme any-data Сенсоры Высота 15 addr[0x25]"]
[null,"Кнопки",null,null,null,null,null,null,null,null,null,null,null,null,null,null," Кнопки"]
[null,"button-out","button-out","toggle","Кнопки","Свет",1,null,"pin[12]",null,null,"inv[0]","st[0]",null,0,null," button-out light1 toggle Кнопки Свет 1 pin[12] inv[0] st[0]"]
[null,"button-in","button-in","anydata","Охрана","Датчик.движения",2,null,"pin[2]",null,null,null,"st[0]","db[20]",0,null," button-in sensor1 anydata Охрана Датчик.движения 2 pin[2] st[0] db[20]"]
[null,"pwm-out","pwm-out","range","Ползунки","Яркость",3,null,"pin[13]",null,null,null,null,null,0,null," pwm-out light2 range Ползунки Яркость 3 pin[13]"]
[null,"Ввод",null,null,null,null,null,null,null,null,null,null,null,null,null,null," Ввод"]
[null,"input-digit","input-digit","inputDigit","Ввод","Введите.значение",1,null,null,null,null,null,"st[60]",null,0,null," input-digit value1 inputDigit Ввод Введите.значение 1 st[60]"]
[null,"input-time","input-time","inputTime","Ввод","Введите.время",2,null,null,null,null,null,"st[13-00-00]",null,0,null," input-time time1 inputTime Ввод Введите.время 2 st[13-00-00]"]
[null,"Вывод",null,null,null,null,null,null,null,null,null,null,null,null,null,null," Вывод"]
[null,"output-text","text1","anydata","Вывод","Текст",1,null,null,null,null,null,"st[hello]",null,0,null," output-text text1 anydata Вывод Текст 1 st[hello]"]
[null,"Исполнительные устройства",null,null,null,null,null,null,null,null,null,null,null,null,null,null," Исполнительные устройства"]
[null,"servo","servo1","range","Сервы",null,1,null,"pin[12]","map[1,100,1,100]",null,null,"st[90]",null,0,null," servo servo1 range Сервы 1 pin[12] map[1,100,1,100] st[90]"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]